# Software Information
display_name = "Fairchild ChannelF (FreeChaF)"
authors = "David Richardson"
supported_extensions = "bin|chf"
corename = "FreeChaF"
license = "GPLv3"
permissions = ""
display_version = "GIT"
categories = "Emulator"

# Hardware Information
manufacturer = "Fairchild"
systemname = "FreeChaF"

# Libretro Information
database = "FreeChaF"
supports_no_game = "false"
firmware_count = 3
firmware0_desc = "sl31253.bin"
firmware0_path = "sl31253.bin"
firmware0_opt = "false"
firmware1_desc = "sl31254.bin"
firmware1_path = "sl31254.bin"
firmware1_opt = "false"
firmware2_desc = "sl90025.bin"
firmware2_path = "sl90025.bin"
firmware2_opt = "false"
notes = "(!) sl31253.bin (md5): ac9804d4c0e9d07e33472e3726ed15c3|(!) sl31254.bin (md5): da98f4bb3242ab80d76629021bb27585|(!) sl90025.bin (md5): 95d339631d867c8f1d15a5f2ec26069d"

description = "A lightweight Fairchild ChannelF / Video Entertainment System designed for libretro. This core was written specifically for use with low-power devices, such as Raspberry Pi, and supports loading a 'no cart' ROM to play the built-in games, controller swapping and dual-analog controls. The core requires the sl31253 and sl31254 BIOS images but the sl90025 BIOS will supersede the sl31253 version if found."
